# Quick Start Guide

[**简体中文**](README_zh.md) | [**English**](README.md)

## Linux Kernel Requirement

## Kernel Version

Use `uname -r` to check the kernel version on your machine.

> **Note**
> If you find your kernel version is `< 5.8`, follow the [**Upgrade Guide**](./kernel-upgrade.md) to upgrade the kernel to the minimum required version.

**Bind to LAN: >= 5.8**

You need bind dae to LAN interface, if you want to provide network service for LAN as an intermediate device.

This feature requires the kernel version of machine on which dae install >= 5.8.

Note that if you bind dae to LAN only, dae only provide network service for traffic from LAN, and not impact local programs.

**Bind to WAN: >= 5.8**

You need bind dae to WAN interface, if you want dae to provide network service for local programs.

This feature requires kernel version of the machine >= 5.8.

Note that if you bind dae to WAN only, dae only provide network service for local programs and not impact traffic coming in from other interfaces.

## Kernel Configurations

Usually, mainstream desktop distributions have these items turned on. But in order to reduce kernel size, some items are turned off by default on embedded device distributions like OpenWRT, Armbian, etc.

Use following command to show kernel configuration items on your machine.

```shell
zcat /proc/config.gz || cat /boot/{config,config-$(uname -r)}
```

dae needs:
```
CONFIG_BPF=y
CONFIG_BPF_SYSCALL=y
CONFIG_BPF_JIT=y
CONFIG_CGROUPS=y
CONFIG_KPROBES=y
CONFIG_NET_INGRESS=y
CONFIG_NET_EGRESS=y
CONFIG_NET_SCH_INGRESS=m
CONFIG_NET_CLS_BPF=m
CONFIG_NET_CLS_ACT=y
CONFIG_BPF_STREAM_PARSER=y
CONFIG_DEBUG_INFO=y
# CONFIG_DEBUG_INFO_REDUCED is not set
CONFIG_DEBUG_INFO_BTF=y
CONFIG_KPROBE_EVENTS=y
CONFIG_BPF_EVENTS=y
```
Check them using command like:

```shell
(zcat /proc/config.gz || cat /boot/{config,config-$(uname -r)}) | grep -E 'CONFIG_(DEBUG_INFO|DEBUG_INFO_BTF|KPROBES|KPROBE_EVENTS|BPF|BPF_SYSCALL|BPF_JIT|BPF_STREAM_PARSER|NET_CLS_ACT|NET_SCH_INGRESS|NET_INGRESS|NET_EGRESS|NET_CLS_BPF|BPF_EVENTS|CGROUPS)=|# CONFIG_DEBUG_INFO_REDUCED is not set'
```

> **Note**
> `Armbian` users can follow the [**Upgrade Guide**](./kernel-upgrade.md) to upgrade the kernel to meet the kernel configuration requirement.

## Installation

### Archlinux/Manjaro

dae has been released on [AUR](https://aur.archlinux.org/packages/dae/).

```shell
# yay -S dae
pacman -S --needed git base-devel
git clone https://aur.archlinux.org/dae.git
cd dae
makepkg -si
```

After installation, use systemctl to control it.

```shell
# start dae
sudo systemctl start dae

# auto start dae at boot
sudo systemctl enable dae
```

### Docker

Pre-built image and related docs can be found at https://hub.docker.com/r/daeuniverse/dae.

Alternatively, you can use `docker compose`:

```shell
git clone --depth=1 https://github.com/daeuniverse/dae
docker compose up -d --build
```

### Installation Script

See [daeuniverse/dae-installer](https://github.com/daeuniverse/dae-installer) (or [mirror](https://hubmirror.v2raya.org/daeuniverse/dae-installer)).

### Build from scratch

See [Build Guide](build-by-yourself.md).

## Minimal Configuration

For minimal bootable config:

```shell
global{}
routing{}
```

However, this config leaves dae no-load state. If you want dae to be in working state, following is a best practice for small config:

```shell
global {
  # Bind to LAN and/or WAN as you want. Replace the interface name to your own.
  #lan_interface: docker0
  wan_interface: auto # Use "auto" to auto detect WAN interface.

  log_level: info
  allow_insecure: false
  auto_config_kernel_parameter: true
}

subscription {
  # Fill in your subscription links here.
}

# See https://github.com/daeuniverse/dae/blob/main/docs/dns.md for full examples.
dns {
  upstream {
    googledns: 'tcp+udp://dns.google.com:53'
    alidns: 'udp://dns.alidns.com:53'
  }
  routing {
    request {
      fallback: alidns
    }
    response {
      upstream(googledns) -> accept
      !qname(geosite:cn) && ip(geoip:private) -> googledns
      fallback: accept
    }
  }
}

group {
  proxy {
    #filter: name(keyword: HK, keyword: SG)
    policy: min_moving_avg
  }
}

# See https://github.com/daeuniverse/dae/blob/main/docs/routing.md for full examples.
routing {
  pname(NetworkManager) -> direct
  dip(224.0.0.0/3, 'ff00::/8') -> direct

  ### Write your rules below.

  dip(geoip:private) -> direct
  dip(geoip:cn) -> direct
  domain(geosite:cn) -> direct

  fallback: proxy
}
```

See more at [example.dae](https://github.com/daeuniverse/dae/blob/main/example.dae).

If you use PVE, refer to [#37](https://github.com/daeuniverse/dae/discussions/37).

## Reload and suspend

When the configuration changes, it is convenient to use command to hot reload the configuration, and the existing connection will not be interrupted in the process. When you want to suspend dae, you can use command to pause.

See [Reload and suspend](reload-and-suspend.md).

## Troubleshooting

See [Troubleshooting](troubleshooting.md).
